To install Levenhuk ToupView(R) software, please follow these steps:

1. For Windows OS:

- Run this file: autorun.exe.
- Click the "Install Image Software" button to install
Levenhuk ToupView(R) application for Windows.
- Click the "Advanced User Manual" button to view the
detailed user manual in English, or browse the CD.
- Click the "Basic User Manual" button to view the
QuickStart in Russian, or browse the CD.
- User Manual for your Levenhuk camera is available in the Manuals
folder.
- Click the "Install DirectShow Driver" button to install 
DirectShow driver for 3rd-party software or for development.
- Click the "Install Twain Driver" button to install Twain
driver for 3rd-party software or for development.  

2. For Mac OS:

- Locate the ToupViewX_Mac folder on your CD. Run the
ToupViewX.dmg file to install Levenhuk ToupViewX(R) application for Mac OS.
- The Manuals folder includes the detailed user manual in
English, the QuickStart in Russian and the user manual for
your Levenhuk camera.

3. For Linux:
- Locate the ToupViewX_Linux folder on your CD. Unpack the
ToupViewX.tar.gz file and run the installation file to install
Levenhuk ToupViewX(R) application for Linux.
Basically, this driver was compiled on Ubuntu 10.04 with kernel 
2.6.32-50-generic-pae. In case if you need assistance using 
this product please contact your local Levenhuk branch.
- The Manuals folder includes the detailed user manual in
English, the QuickStart in Russian and the user manual for
your Levenhuk camera.

(c) 2006-2015 Levenhuk, Inc. USA
====